**Aerospace, Android and Windows 8 Coordinate Systems**

**(orientation.c)**

**Technical Note**

Document TBD

Version: Draft

Authors: Mark Pedley and Michael Stanley

Date: September 2014

Table of Contents

[1 Introduction 4](#_Toc395011626)

[1.1 Summary 4](#_Toc395011627)

[1.2 Axes Definitions 4](#_Toc395011628)

[1.3 Euler Angle Orientation Matrix 5](#_Toc395011629)

[1.4 Gimbal Lock 5](#_Toc395011630)

[1.5 Euler Angle Discontinuities 5](#_Toc395011631)

[1.6 Functions 6](#_Toc395011632)

[2 Aerospace (NED) Coordinate System 8](#_Toc395011633)

[2.1 Axis Definitions 8](#_Toc395011634)

[2.2 Orientation Matrix in terms of Euler Angles 8](#_Toc395011635)

[2.3 Orientation Quaternion in terms of Euler Angles 9](#_Toc395011636)

[2.4 Gimbal Lock 9](#_Toc395011637)

[2.5 Euler Angle Discontinuities 10](#_Toc395011638)

[2.6 Calculation of Euler Angles From Rotation Matrix 12](#_Toc395011639)

[3 Android Coordinate System 14](#_Toc395011640)

[3.1 Axes 14](#_Toc395011641)

[3.2 Orientation Matrix in terms of Euler Angles 15](#_Toc395011642)

[3.3 Orientation Quaternion in terms of Euler Angles 15](#_Toc395011643)

[3.4 Gimbal Lock 16](#_Toc395011644)

[3.5 Euler Angle Discontinuities 16](#_Toc395011645)

[3.6 Calculation of Euler Angles From Rotation Matrix 18](#_Toc395011646)

[4 Windows 8 Coordinate System 20](#_Toc395011647)

[4.1 Axes 20](#_Toc395011648)

[4.2 Orientation Matrix in terms of Euler Angles 21](#_Toc395011649)

[4.3 Orientation Quaternion in terms of Euler Angles 21](#_Toc395011650)

[4.4 Gimbal Lock 22](#_Toc395011651)

[4.5 Euler Angle Discontinuities 22](#_Toc395011652)

[4.6 Calculation of Euler Angles From Rotation Matrix 25](#_Toc395011653)

**Glossary**

General quaternion

Rotation matrix

Aerospace (NED) rotation matrix

Android rotation matrix

Windows 8 rotation matrix

Rotation matrix about x axis

Rotation matrix about y axis

Rotation matrix about z axis

Pitch angle

*ρ*Compass heading angle

Roll angle

Tilt angle

*ψ* Yaw angle

## Introduction

### Summary

This Application Note documents the three coordinate systems used in Freescale's Sensor Fusion software:

- Aerospace (a x=North, y=East, z=Down or NED standard)

- Android (a x=East, y=North, z=Up or ENU standard)

- Windows 8 (another x=East, y=North, z=Up or ENU standard)

If developing for Android or Windows 8 systems then your choice is made for you. If not, the Aerospace coordinate system is probably the best choice since its sequence of rotations and ranges of Euler angles lead to a yaw/compass heading estimate that is more ergonomic than those computed from the other coordinate systems. Specifically, a 180o roll while the system is pointed northwards (but inverted) results in an unchanged northwards yaw/compass heading and a 180o pitch rotation (so the system is pointing south but inverted) leads to a southwards yaw/compass heading in the Aerospace coordinate system. The reverse occurs in the Android and Windows 8 coordinate systems.

### Axes Definitions

Sections 2.1, 3.1 and 4.1 define the axes, the sign standard for the accelerometer and the definition of a positive rotation about any axis for the Aerospace, Android and Windows 8 coordinate systems.

Accelerometers measure linear acceleration minus the gravity component in each axis. This is a consequence of basic Physics which states the equivalence between the forces experienced when at rest in a gravitational field and when accelerating in the opposite direction. The author is writing this document sitting on a chair at rest in a 1g downwards pointing gravitational field but would experience exactly the same forces sitting in a spaceship with a 1g rocket engine providing a 1g acceleration towards the cabin ceiling.

The Aerospace and Windows 8 coordinate systems are gravity positive meaning that an accelerometer axis measures +1g when pointed downwards and aligned with gravity. The Android coordinate system is acceleration positive meaning that an acceleration axis measures +1g when pointed upwards and aligned with the equivalent 1g acceleration in the opposite direction to gravity.

The Aerospace and Windows 8 coordinate systems define rotations in the usual mathematical sense that a rotation is positive when it has a clockwise sense when viewed in the increasing direction of an axis. Rotations in the Android coordinate system have the opposite sign probably as a result of a bug in an early Android specification which became too expensive to fix later.

|  |  |  |  |
| --- | --- | --- | --- |
| **Item** | **Aerospace (NED)** | **Android (ENU)** | **Windows 8 (ENU)** |
| Axes alignment | XYZ=NED | XYZ=ENU | XY=ENU |
| Accelerometer sign | Gravity-Acceleration  +1g when axis down  -1g when axis is up | Acceleration-Gravity  +1g when axis up  -1g when axis is down | Gravity-Acceleration  +1g when axis down  -1g when axis is up |
| Accelerometer reading when flat | G[Z]=+1g | G[Z]=+1g | G[Z]=-1g |
| Direction of positive rotations | Clockwise sense | Anti-clockwise sense | Clockwise sense |
| Compass heading *ρ* | *ρ=ψ* | *ρ=ψ* | *ρ*=360o-*ψ* |

### Euler Angle Orientation Matrix

Orientation matrices and quaternions are independent of assumptions about the Euler angles (roll, pitch and yaw) and the order in which the Euler angle rotations are applied. Euler angles have poor mathematical properties and are only used in Freescale's Sensor Fusion software as an output for human consumption. Euler angles have many problems of which one is that rotation matrices do not commute and order in which individual Euler angle rotations are applied is important. With different assumptions about the order of individual Euler angle rotations the same orientation matrix will give different roll, pitch and yaw angles.

Since the three standards require the Euler angles to be computed, the table below lists the decomposition of the orientation matrix into three Euler angle rotation matrices in the three standards. As mentioned in section 1.2, pitching the far end of a product upwards in the Aerospace and Windows 8 coordinate systems gives a positive pitch and a negative pitch in the Android standard.

|  |  |  |  |
| --- | --- | --- | --- |
| **Item** | **Aerospace (NED)** | **Android (ENU)** | **Windows 8 (ENU)** |
| Sequence of Euler angle rotations |  |  |  |

### Gimbal Lock

Gimbal lock occurs in all three coordinate systems when the second rotation (pitch in Aerospace and Windows 8, roll in Android) aligns the axes of the first and third Euler angle rotations. The number of degrees of freedom reduces from 3 Euler angles to just 2 Euler angles needed to define the orientation. Any change in the first Euler angle can be offset by a cancelling change in the third Euler angle and the two oscillate unstably together.

Gimbal lock in software strapdown navigation systems is therefore an avoidable mathematical instability that results purely from the decomposition of the orientation matrix or quaternion into three individual Euler angle rotations. The orientation matrix or quaternion itself is completely stable at gimbal lock orientations.

Freescale's Sensor Fusion software uses orientation matrix and quaternion algebra throughout and only computes Euler angles for human use as an output from the algorithms. The computed orientation is therefore just as stable at gimbal lock orientations as at other orientations. Gimbal lock is not a problem with Freescale's software. Any software which is based on Euler angle rotations in preference to rotation matrix or quaternion will suffer gimbal lock instability and other discontinuities discussed next.

|  |  |  |  |
| --- | --- | --- | --- |
| **Item** | **Aerospace (NED)** | **Android (ENU)** | **Windows 8 (ENU)** |
| Gimbal lock | +/- 90o pitch (y axis) | +/- 90o roll (y axis) | +/- 90o pitch (x axis) |

### Euler Angle Discontinuities

Another problem with Euler angle representation of orientation is that in addition to their being an infinite number of Euler angle solutions at gimbal lock orientations, there are two Euler angle solutions for all other orientations. This forces one of the Euler angles to be constrained with a reduced range of just -90o to +90o to eliminate one of the two solutions.

The presence of two solutions is easily demonstrated with the starting position of the PCB flat on the table and then applying these two rotation sequences: i) a rotation of 180o in pitch and ii) a rotation of 180o in yaw followed by a rotation of 180o in pitch. Both result in the same orientation. Given that orientation, both Euler angle representations give the same orientation matrix and quaternion.

The Aerospace coordinate system restricts the range of the pitch angle from -90o to +90o. The Android and Windows 9 coordinate systems restrict the range of roll angle from -90o to +90o. Although this restriction results in just one Euler angle solution at all orientations except at gimbal lock, it creates the unfortunate mathematical side-effect of introducing additional discontinuities in the Euler angles at -90o and +90o in the Aerospace coordinate system and at -90o and +90o roll angles in the Android and Windows 8 coordinate systems. Although this occurs at the same orientation as gimbal lock in the Aerospace and Android coordinate systems, it is a different phenomenon as shown by it occurring at a different orientation (-90o and +90o roll) compared to gimbal lock (-90o and +90o pitch) in the Windows 8 coordinate system.

At the further risk of repetition, Euler angles are mathematically troublesome and must be avoided in the inner workings of strapdown sensor fusion software. Their only role is providing output to humans as specified by the Android, Windows 8 or other standard.

The table below summarizes the Euler angle discontinuities in each coordinate system. The meanings of the various entries will become clearer after reading sections 2 through 4.

|  |  |  |  |
| --- | --- | --- | --- |
| **Item** | **Aerospace (NED)** | **Android (ENU)** | **Windows 8 (ENU)** |
| Ranges of Euler angles | 0o ≤ Yaw *ψ* (*z*) < 360o  -90o ≤ Pitch *θ* (*y*) < 90o  -180o ≤ Roll *φ* (*x*) < 180o | 0o ≤ Yaw *ψ* (*z*) < 360o  -90o ≤ Roll *φ* (*y*) < 90o  -180o ≤ Pitch *θ* (*x*) < 180o | 0o ≤ Yaw *ψ* (*z*) < 360o  -180o ≤ Pitch *θ* (*x*) < 180o  -90o ≤ Roll *φ* (*y*) < 90o |
| Equivalent matrix |  |  |  |
| Behavior during +/- 180 deg roll rotation | Roll is continuous in range -180o to 180o.  No change in yaw or compass angle. | Roll is continuous increasing to 90o and then decreasing or decreasing to -90o and then increasing.  Pitch and yaw have 180o discontinuities at +/-90o roll. | 180o jump in roll, pitch, yaw and compass as the roll angle passes 90o and -90o. |
| Behavior during +/- 180 deg pitch rotation | Pitch is continuous increasing to 90o and then decreasing or decreasing to -90o and then increasing.  Roll and yaw have 180o discontinuity at +/-90o pitch. | Smooth changes in pitch. No change in roll, yaw or compass. | Smooth changes in pitch. No change in roll, yaw or compass. |

### Functions

|  |
| --- |
| void fNEDAnglesDegFromRotationMatrix(float R[][3], float \*pfPhiDeg, float \*pfTheDeg, float \*pfPsiDeg,  float \*pfRhoDeg, float \*pfChiDeg);  Computes the roll, pitch, yaw, compass heading and tilt angles from an Aerospace/NED orientation matrix.  See section 2.1. |
| void fAndroidAnglesDegFromRotationMatrix(float R[][3], float \*pfPhiDeg, float \*pfTheDeg, float \*pfPsiDeg,  float \*pfRhoDeg, float \*pfChiDeg);  Computes the roll, pitch, yaw, compass heading and tilt angles from an Aerospace/NED orientation matrix.  See section 2.2. |
| void fWin8AnglesDegFromRotationMatrix(float R[][3], float \*pfPhiDeg, float \*pfTheDeg, float \*pfPsiDeg,  float \*pfRhoDeg, float \*pfChiDeg);  Computes the roll, pitch, yaw, compass heading and tilt angles from an Aerospace/NED orientation matrix.  See section 2.3. |

## Aerospace (NED) Coordinate System

### Axis Definitions

The Aerospace coordinate system is shown in Figure 4-1. It is an x=North, y=East, z=Down (termed NED) coordinate system meaning that when the product is in its default orientation lying flat on the table and pointed northwards, the x axis points north, the y axis points east and the z axis points downwards.

The sign of rotations about the x, y and z axes is defined in the normal mathematical sense that a clockwise rotation is deemed positive when looking along the increasing direction of the axis. Roll, pitch and yaw rotations have their normal meaning and therefore correspond to rotations about the x, y and z axes respectively. The yaw angle equals the compass angle .

The Aerospace coordinate system is gravity (not acceleration) positive meaning that the output of any accelerometer channel is positive when pointing downwards and aligned with gravity. The accelerometer *z* axis reading is therefore +1g when the phone is flat and upright.



Figure 2-1: The Aerospace (NED) Coordinate System

### Orientation Matrix in terms of Euler Angles

The sequence of Euler angle rotations in the Aerospace coordinate system is i) first yaw ii) secondly pitch and iii) finally roll. The roll rotation is about the x axis, the pitch rotation about the y axis and the yaw rotation about the z axis. The individual rotation matrices are:

Eq 2.2.1

Eq 2.2.2

Eq 2.2.3

The composite Aerospace rotation matrix using the specified rotation sequence is then:

Eq 2.2.4

Eq 2.2.5

### Orientation Quaternion in terms of Euler Angles

The individual Euler angle rotation quaternions in the Aerospace coordinate system are:

Eq 2.3.1

Eq 2.3.2

Eq 2.3.3

The Aerospace rotation quaternion evaluates to:

Eq 2.3.4

Eq 2.3.5

The elements of the Aerospace quaternion are therefore:

Eq 2.3.6

Eq 2.3.7

Eq 2.3.8

Eq 2.3.9

### Gimbal Lock

Gimbal lock occurs in the Aerospace coordinate system when the second pitch rotation aligns the first yaw and third roll rotations. This occurs at 90o pitch upwards and 90o pitch downwards. The number of degrees of freedom in the Euler angle description of the orientation therefore reduces from 3 to 2 and the roll and yaw angle oscillate with only their sum and difference defined.

At gimbal lock and , equation 2.2.5 simplifies to:

Eq 2.4.1

Eq 2.4.2

The orientation matrix is stable but the differenced angle or the summed angle can be determined at the two gimbal lock orientations.

### Euler Angle Discontinuities

The Aerospace rotation matrix is equal to the matrix where radians corresponds to 180 degrees. By direct evaluation:

Eq 2.5.1

Eq 2.5.2

This is the mathematical identity equivalent to the statement made in section 1 that there are two Euler angle solutions to each orientation. In words: "As an alternative to a rotation of in yaw then in pitch and finally by in roll, I can get to the same orientation by rotating 180o plus in yaw, then 180o minus in pitch and finally by 180o plus in roll."

The Aerospace coordinate system removes one of the two solutions by restricting the pitch angle to the range -90o to +90o. Equations 2.5.1 and 2.5.2 then state that whenever the pitch angle is above 90o or less than -90o then the roll angle should increase by 180o (the term), the pitch angle should be negated and 180o added (the term) and the yaw/compass heading should increase by 180o (the term). These discontinuities are shown in Figure 2-2 to 2-4.

Figure 2-2 shows the Euler angles as the PCB is rotated through 360o in roll from the default starting position of being flat and pointed northwards. Neither the pitch nor yaw angles change and the roll discontinuity from -180o to +180o is simply a consequence of modulo 360o arithmetic and is quite acceptable. The average user of a smartphone eCompass will agree that if a smartphone is pointed northwards and then given a roll rotation of 180o then it is still pointed northwards.

Figure 2-3 shows the Euler angles as the PCB is rotated 360o in pitch from the same starting position. The pitch angle reaches 90o and then starts smoothly decreasing without a discontinuity until it reaches -90o and then starts increasing smoothly. The yaw/compass angle flips by 180o at the 90o and -90o pitch angles but this is reasonable ergonomic behavior. For the same reasons discussed above, the average smartphone user will consider a 180o pitch rotation to flip the yaw/compass heading 180o.

Figure 2-4 shows the yaw/compass angle behavior as the PCB is rotated 360o in yaw while remaining flat. The yaw/compass heading increases smoothly with the acceptable modulo 360o discontinuity when pointed northwards.

This relatively benign behavior is the justification for the comment made in Section 1 that the Aerospace coordinate system is the most ergonomically reasonable and should be used in preference unless specifically developing for the Android and Windows 8 standards.



Figure 2-2: 360 degree roll rotation at zero pitch and yaw in the NED coordinate system



Figure 2-3: 360 degree pitch rotation at zero roll and yaw in the NED coordinate system



Figure 2-4: 360 degree yaw rotation at zero roll and pitch in the NED coordinate system

### Calculation of Euler Angles From Rotation Matrix

This section documents function fNEDAnglesDegFromRotationMatrix which computes the Euler angles from the Aerospace rotation matrix as defined in equation 2.2.5:

The solution for the three Aerospace Euler angles is:

Eq 2.6.1

Eq 2.6.2

Eq 2.6.3

The Aerospace compass heading angle always equals the yaw angle :

Eq 2.6.4

At gimbal lock, equations 2.4.1 and 2.4.2 give:

Eq 2.6.5

Eq 2.6.6

The tilt angle from vertical can be determined from the scalar product of the rotated gravity vector and the downwards z axis giving:

Eq 2.6.7

## Android Coordinate System

### Axes

The reference for this section is the Android specification available at:

http://developer.android.com/reference/android/hardware/SensorEvent.html

*Android: "The coordinate space is defined relative to the screen of the phone in its default orientation. The axes are not swapped when the device's screen orientation changes. The OpenGL ES coordinate system is used. The origin is in the lower-left corner with respect to the screen, with the X axis horizontal and pointing right, the Y axis vertical and pointing up and the Z axis pointing outside the front face of the screen. In this system, coordinates behind the screen have negative Z values."*

The Android sensor coordinate system is shown in Figure 5-1. It is an x=East, y=North, z=Up (termed ENU) coordinate system meaning that when the product is in its default orientation lying flat on the table and pointed northwards, the x axis points east, the y axis points north and the z axis points upwards.

The sign of rotations about the x, y and z axes is defined as the opposite to normal mathematical sense. An anti-clockwise rotation is deemed positive when looking along the increasing direction of the axis. Roll, pitch and yaw rotations have their normal meaning and therefore correspond to rotations about the y, x and z axes respectively. The yaw angle equals the compass angle .

The Android coordinate system is acceleration (not gravity) positive meaning that the output of any accelerometer channel is positive when pointing upwards and aligned against gravity. The accelerometer *z* axis reading is therefore +1g when the product is flat and upright. This is the same as in the Aerospace coordinate system as a result of two cancelling sign changes: i) the z axes point in opposite directions and ii) Aerospace is gravity positive and Android is acceleration positive.

*Android: "When the device lies flat on a table, the acceleration value is +9.81, which correspond to the acceleration of the device (0 m/s^2) minus the force of gravity"*



Figure 3-1: The Android Coordinate System

### Orientation Matrix in terms of Euler Angles

The sequence of Euler angle rotations in the Android coordinate system does not appear to be documented in the standard. Investigation of the behavior of Android tablets and phones indicates that most use i) first yaw ii) secondly roll and iii) finally pitch. The roll rotation is about the y axis, the pitch rotation about the x axis and the yaw rotation about the z axis. The individual rotation matrices are:

Eq 3.2.1

Eq 3.2.2

Eq 3.2.3

The composite Android rotation matrix using the specified rotation sequence is:

Eq 3.2.4

Eq 3.2.5

### Orientation Quaternion in terms of Euler Angles

The individual Euler angle rotation quaternions in the Android coordinate system are:

Eq 3.3.1

Eq 3.3.2

Eq 3.3.3

The Android rotation quaternion evaluates to:

Eq 3.3.4

Eq 3.3.5

The elements of the Android quaternion are therefore:

Eq 3.3.6

Eq 3.3.7

Eq 3.3.8

Eq 3.3.9

### Gimbal Lock

Gimbal lock occurs in the Android coordinate system when the second roll rotation aligns the first yaw and third pitch rotations. This occurs at +90o roll and -90o roll. The number of degrees of freedom in the Euler angle description of the orientation therefore reduces from 3 to 2 and the pitch and yaw angles oscillate with only their sum and difference defined.

At gimbal lock , equation 3.2.5 simplifies to:

Eq 3.4.1

At gimbal lock , equation 3.2.5 simplifies to:

Eq 3.4,2

The orientation matrix is stable but the summed angle or the differences angle can be determined at the two gimbal lock orientations.

### Euler Angle Discontinuities

The Android rotation matrix is equivalent to the matrix . By direct evaluation:

Eq 3.5.1

Eq 3.5.2

Equation 3.5.1 and 3.5.2 show that there are two solutions for the Android Euler angles for a given rotation matrix. If and are one solution for the roll, pitch and yaw angles for a given orientation matrix, then so is the solution given by roll angle 180o minus , pitch angle 180o plus and yaw angle 180o plus .

The Android specification removes of the two solutions by restricting the roll angle to the range -90o to +90o.

***"***[***Sensor.TYPE\_ORIENTATION***](http://developer.android.com/reference/android/hardware/Sensor.html#TYPE_ORIENTATION)***:***

*"All values are angles in degrees.*

*values[0]: Azimuth, angle between the magnetic north direction and the Y axis, around the Z axis (0 to 359). 0=North, 90=East, 180=South, 270=West*

*values[1]: Pitch, rotation around X axis (-180 to 180), with positive values when the z-axis moves toward the y-axis.*

*values[2]: Roll, rotation around Y axis (-90 to 90), with positive values when the x-axis moves toward the z-axis."*

Equations 3.5.1 and 3.5.2 then state that whenever the roll angle is above 90o or less than -90o then the pitch angle should increase by 180o (the term), the roll angle should be negated and 180o added (the term) and the yaw/compass heading should increase by 180o (the term). These discontinuities are shown in Figure 3-2 to 3-4.

Figure 3-2 shows the Euler angles as the PCB is rotated through 360o in roll from the default starting position of being flat and pointed northwards. The roll angle reaches 90o and then starts smoothly decreasing without a discontinuity until it reaches -90o and then starts increasing smoothly. The yaw/compass angle flips by 180o at the 90o and -90o roll angles.

Figure 3-3 shows the Euler angles as the PCB is rotated 360o in pitch from the same starting position. The pitch angle increases smoothly with the acceptable modulo 360o discontinuity between the equivalent angles of -180o and +180o.

Figure 3-4 shows the yaw/compass angle behavior as the PCB is rotated 360o in yaw while remaining flat. The yaw/compass heading increases smoothly with the acceptable modulo 360o discontinuity when pointed northwards.

The 180o compass heading change when the Android roll angle passes through -90o or +90o is arguably not ideal from an ergonomic standpoint. The average user would probably say that given an initial starting point pointing northwards then i) after a 180o roll rotation it is still pointing northwards (Android says it now points southwards) and ii) after a 180o pitch rotation it is pointing southwards (Android says it is still pointing northwards).



Figure 3-2: 360 degree roll rotation at zero pitch and yaw in the Android coordinate system



Figure 3-3: 360 degree pitch rotation at zero roll and yaw in the Android coordinate system



Figure 3-4: 360 degree yaw rotation at zero roll and pitch in the Android coordinate system

### Calculation of Euler Angles From Rotation Matrix

This section documents function fAndroidAnglesDegFromRotationMatrix which computes the Euler angles from the Android rotation matrix as defined in equation 3.2.5:

The solution for the three Android Euler angles is:

Eq 3.6.1

Eq 3.6.2

Eq 3.6.3

The Android compass heading angle always equals the yaw angle :

Eq 3.6.4

At gimbal lock equations 3.4.1 and 3.4.2 give:

Eq 3.6.5

Eq 3.6.6

The tilt angle from vertical can be determined from the scalar product of the rotated gravity vector and the downwards z axis giving:

Eq 3.6.7

## Windows 8 Coordinate System

### Axes

The reference for this section is the Microsoft specification:

"Integrating Motion and Orientation Sensors"

available for download at:

<http://msdn.microsoft.com/en-us/library/windows/hardware/dn642102(v=vs.85).aspx>

The Windows 8 coordinate system is shown in Figure 4-1. It is an x=East, y=North, z=Up (termed ENU) coordinate system like Android.

The sign of rotations about the x, y, and z axes is opposite to Android and therefore compatible with normal mathematical usage. A consequence is that the Windows 8 compass heading angle has the opposite sense to the Windows 8 yaw angle and .

The Windows 8 coordinate system is gravity (not acceleration) positive meaning that the output of any accelerometer channel is negative when pointing upwards and aligned against gravity. The accelerometer z axis reading is therefore -1g when the product is flat and upright.

*Microsoft: "a. Lay the device on a flat surface with the screen pointing up – acceleration values should be the following:*

*X = ~0.0, Y = ~0.0, Z = ~-1.0*

*b. Hold the device with the right hand side pointing upwards up – acceleration values should be the following:*

*X = ~-1.0, Y = ~0.0, Z = ~0.0*

*c. Hold the device with the top of the screen pointing upwards up – acceleration values should be the following:*

*X = ~0.0, Y = ~-1.0, Z = ~0.0"*



Figure 6-1: Windows 8 Coordinate System

### Orientation Matrix in terms of Euler Angles

The order of the rotations in Windows 8 matches the Aerospace standard but not Android. The yaw rotation is first, followed by pitch rotation and then followed by a roll rotation.

*Microsoft: "In order to properly describe the orientation of the device in 3D-space, the Euler angles are applied in the following order, starting with the device lying on a flat surface and the +Y axis pointing due North (towards the North Pole):*

*1. The device is rotated by the Yaw angle about its Z-axis (opposite rotation direction about Z-axis compared to heading).*

*2. The device is rotated by the Pitch angle about its X-axis.*

*3. The device is rotated by the Roll angle about its Y-axis."*

The individual Windows rotation matrices are:

Eq 4.2.1

Eq 4.2.2

Eq 4.2.3

The composite Windows 8 rotation matrix using the Microsoft rotation sequence is:

Eq 4.2.4

Eq 4.2.5

### Orientation Quaternion in terms of Euler Angles

The individual Euler angle rotation quaternions in the Windows 8 coordinate system are:

Eq 4.3.1

Eq 4.3.2

Eq 4.3.3

The Windows 8 rotation quaternion evaluates to:

Eq 4.3.4

Eq 4.3.5

The elements of the Windows 8 quaternion are therefore:

Eq 4.3.6

Eq 4.3.7

Eq 4.3.8

Eq 4.3.9

### Gimbal Lock

Gimbal lock occurs in the Windows 8 coordinate system when the second pitch rotation aligns the first yaw and third roll rotations. This occurs at +90o pitch and -90o pitch angles. The number of degrees of freedom in the Euler angle description of the orientation therefore reduces from 3 to 2 and the roll and yaw angles oscillate with only their sum and difference defined.

At gimbal lock , equation 4.2.5 simplifies to:

Eq 4.4.1

At gimbal lock , equation 4.2.5 simplifies to:

Eq 4.4.2

The orientation matrix is stable but only the summed angle or the differenced angle can be determined at the two gimbal lock orientations.

### Euler Angle Discontinuities

The Windows 8 rotation matrix is equal to the matrix . By direct evaluation:

Eq 4.5.1

Eq 4.5.2

Equation 4.5.1 and 4.5.2 show that there are two solutions for the Windows 8 Euler angles for a given rotation matrix. If and are one solution for the roll, pitch and yaw angles for a given orientation matrix, then so is the solution given by roll angle 180o plus , pitch angle 180o minus and yaw angle 180o plus .

The Windows 8 specification removes of the two solutions by restricting the roll angle to the range -90o to +90o.

*Microsoft: "The following ranges are used for the representation of Yaw, Pitch, and Roll:*

*• 0.0° ≤ Yaw < 360.0°*

*• -180.0° ≤ Pitch < 180.0°*

*• -90.0° ≤ Roll < 90.0°"*

Equations 4.5.1 and 4.5.2 then state that whenever the roll angle is above 90o or less than -90o then the roll angle should increase by 180o (the term), the pitch angle should be negated and 180o added (the term) and the yaw/compass heading should increase by 180o (the term). These discontinuities are shown in Figure 4-2 to 4-4 and should be compared with Figure 21 in the Microsoft specification "Integrating Motion and Orientation Sensors".

Figure 3-2 shows the Euler angles as the PCB is rotated through 360o in roll from the default starting position of being flat and pointed northwards. The roll angle reaches 90o, has a discontinuity to -90o, increases to 90o and then has another discontinuity to -90o. The pitch and yaw/compass heading angles suffer 180o discontinuities at 90o and -90o roll angles.

Figure 3-3 shows the Euler angles as the PCB is rotated 360o in pitch from the same starting position. The pitch angle increases smoothly with the acceptable modulo 360o discontinuity between the equivalent angles of -180o and +180o.

Figure 3-4 shows the yaw/compass angle behavior as the PCB is rotated 360o in yaw while remaining flat. The yaw/compass heading increases smoothly with the acceptable modulo 360o discontinuity when pointed northwards.

The 180o compass heading change when the Windows 8 roll angle passes through -90o or +90o is, like Android, arguably not ideal from an ergonomic standpoint. But this behavior is forced mathematically onto the Microsoft specification by the unfortunate properties of Euler angles and the requirement to limit the roll angle range from -90o to +90o.



Figure 4-2: 360 degree roll rotation at zero pitch and yaw in the Windows 8 coordinate system



Figure 4-3: 360 degree pitch rotation at zero roll and yaw in the Windows 8 coordinate system



Figure 4-4: 360 degree yaw rotation at zero roll and pitch in the Windows 8 coordinate system

### Calculation of Euler Angles From Rotation Matrix

This section documents function fWin8AnglesDegFromRotationMatrix which computes the Euler angles from the Windows 8 rotation matrix as defined in equation 4.2.5:

The solution for the roll angle is:

Eq 4.6.1

The pitch angle has range but is first computed in the range -90o to 90o using:

Eq 4.6.2

Since is in the range -90o to 90o, it follows that is non-negative and that has the same sign as and can be used to correct into the range :

Eq 4.6.3

Eq 4.6.4

The general solution for the yaw angle for non-zero is given by:

Eq 4.6.5

At gimbal lock, equations 4.4.1 and 4.4.2 give:

Eq 4.6.6

Eq 4.6.7

The Windows 8 compass heading angle is the negative (modulo 360o) of the yaw angle :

Eq 4.6.8

The tilt angle from vertical can be determined from the scalar product of the rotated gravity vector and the downwards z axis giving:

Eq 4.6.9

### Direction of Windows 8 Rotation Matrix

The Freescale sensor fusion software defines the orientation matrix as transforming a vector from the global to the sensor coordinate frame for all coordinate systems. The rotation matrices and quaternions listed on page 82 of the Microsoft specification are the transpose and conjugate of the Freescale standard and therefore refer to transformation from the sensor frame to the global frame. To convert from one to the other, simply take the conjugate of the quaternion or transpose the matrix.

Information in this document is provided solely to enable system and software implementers to use Freescale Semiconductors products. There are no express or implied copyright licenses granted hereunder to design or fabricate any integrated circuits or integrated circuits based on the information in this document.

Freescale Semiconductor reserves the right to make changes without further notice to any products herein. Freescale Semiconductor makes no warranty, representation, or guarantee regarding the suitability of its products for any particular purpose, nor does Freescale Semiconductor assume any liability arising out of the application or use of any product or circuit, and specifically disclaims any liability, including without limitation consequential or incidental damages. "Typical" parameters that may be provided in Freescale Semiconductor data sheets and/or specifications can and do vary in different applications and actual performance may vary over time. All operating parameters, including "Typicals", must be validated for each customer application by customer's technical experts. Freescale Semiconductor does not convey any license under its patent rights nor the rights of others. Freescale Semiconductor products are not designed, intended, or authorized for use as components in systems intended for surgical implant into the body, or other applications intended to support or sustain life, or for any other application in which failure of the Freescale Semiconductor product could create a situation where personal injury or death may occur. Should Buyer purchase or use Freescale Semiconductor products for any such unintended or unauthorized application,

Buyer shall indemnify Freescale Semiconductor and its officers, employees, subsidiaries, affiliates, and distributors harmless against all claims, costs, damages, and expenses, and reasonable attorney fees arising out of, directly or indirectly, any claim of personal injury or death associated with such unintended or unauthorized use, even if such claims alleges that Freescale Semiconductor was negligent regarding the design or manufacture of the part.

RoHS-compliant and/or Pb-free versions of Freescale products have the functionality and electrical characteristics as their non-RoHS-complaint and/or non-Pb-free counterparts.

For further information, see http://www.freescale.com or contact your Freescale sales representative.

For information on Freescale's Environmental Products program, go to http://www.freescale.com/epp.

Freescale™ and the Freescale logo are trademarks of Freescale Semiconductor, Inc.

All other product or service names are the property of their respective owners.

© 2013 Freescale Semiconductor, Inc.

[Creative Commons License](http://creativecommons.org/licenses/by/4.0/)  
Aerospace, Android and Windows 8 Coordinate Systems by [Freescale Semiconductor](http://www.freescale.com/sensorfusion) is licensed under a [Creative Commons Attribution 4.0 International License](http://creativecommons.org/licenses/by/4.0/).